

SL20S Venetian

Sliding control operated Venetian blind.

This blind is a new version of the manually operated Venetian blind system. It is delivered fully assembled with the external magnet device in place and ready to glaze.

In appearance it has:

* A ‘head rail’ that intrudes approx. 50mm into the sealed unit, the same as the other blind systems. This rail houses the pulleys and cords of the blind operating mechanism.
* A ‘side rail’ that intrudes approx. 50mm into the sealed unit; this houses the internal magnet control that connects through the glass to the external sliding magnet control.
  + The side rail can be either left or right hand side of the unit.
  + There is a transparent guide with top and bottom stops that the external sliding control is fitted to.

Colours

Head rail and side rail: S102 White / S155 Grey / S149 Cream

External magnet colour: S102 White / S155 Grey / S149 Cream

Slat colours: S102 White / S106 Pale Yellow / S125 Beige / S130 Pale Green / S142 Pale Blue

S149 Cream / S155 Grey / S156 Bright (metallic) Silver / S157 Silver

Size details

This differs from other blind types and is absolute.

Minimum width 300mm – Maximum width 1500mm

Minimum height 600mm – Maximum height 2000mm

Width from 300mm – 350mm, maximum height is 1400mm

Width from 351mm – 550mm, maximum height is 1800mm

Width from 551mm – 1500mm, maximum height is 2000mm

**MAXIMUM M2 AREA OF 1.8M2**

Items to specify on ordering:

* Unit dimensions – w x h
* Colour of slat
* Colour of spacer bar – Black or Grey (all spacer is warm edge)
* Colour of head rail, side rail and external sliding magnet control.
* Left or Right side rail control position, from inside view